
***VENNLIGST MERK: INSTALLASJONER SOM IKKE ER UTFØRT RIKTIG, VIL FORÅRSAKE SKADER I TOPPEN PÅ GRUNN AV VANNINNTRENGNING. UTGIFTER FOR ERSTATNING AV TOPPEN VIL BELASTES MONTØREN.***



***VI ANBEFALER AT MONTØREN PRESIST OG FORSIKTIG UTFØRER INSTALLASJONEN SOM ANVIST HER.***

Toppen kommer med et ark som viser den riktige fremgangsmåten for installasjonen.

Dette arket ***må kun fjernes etter installasjonen er fullført i henhold til fremgangsmåten***,

Steg 4.Det er viktig å beskytte toppen med ***papirteip*** for å hindre at overflaten blir skitten;

Steg 5. ***Dette er det viktigste steget for å hindre vanninntrengning.***

Påfør en tykk, nøytral silikongjengetetning (denne må trykkes ut når toppen dyttes mot veggen);

Steg 6. Sett fast med skruer på Melamin / Lakkert / Tretopp II mens den sitter på andre materialer (Ocritech /Tecnoril / Mineralmarmor, osv.), sett fast med nøytralt silikon;

Steg 7. Fjern unødvendig silikon og la en liten bit være igjen på hjørnet;

Steg 8. Fjern papirteipen som sitter igjen på ***VEGG (A) først*** og kun ***etter*** den som sitter på ***TOPP (B)***

(dette hindrer at toppen blir skitten);

***PLEASE MIND: AN INSTALLATION NOT CARRIED OUT PROPERLY WILL CAUSE DAMAGES TO THE TOP DUE TO WATER INFILTRATION. THE COSTS FOR THE TOP REPLACEMENT WILL BE CHARGED TO THE FITTER.***

***WE INVITE THE FITTER TO A CAREFUL AND PRECISE EXECUTION OF THE OPERATION AS HEREWITH SHOWN.***

The Top comes with a sheet illustrating the correct mounting procedure.

This sheet ***must be removed only after the installation is completed,*** following the procedure,

Step 4it's important to protect the Top with ***Paper Tape*** to avoid dirtying the surface;

Step 5 ***this is the most important step to avoid water infiltrations.***

Apply a rich neutral Silicone thread (it has to be squeezed out once the Top is pushed against the wall);

Step 6 fix with screw on Melamine / Lacquered / Wooden Tops II while on top of different materials (Ocritech /Tecnoril / Mineralmarble etc.) fix with neutral silicone;

Step 7 remove the exceeding neutral silicone, leaving a small part on the comer;

Step 8 remove the paper tape stuck on the ***WALL (A) first*** and only ***after*** the one fixed to the ***TOP (B)***

(this way avoiding to dirt the top);